Hasan Tahsin Rafsan

Requirements:

IOT devices (Fan, Light, Door)

Server

PC

Wireless Router

Switch

Procedure

1. First of all I open my Cisco Packet Tracer & logged in
2. Then, I select fan, light, door etc IoT components.
3. Then I took wireless router & then connected them with 2 switches, routers & laptops.
4. On the other hand, I connected wireless connection to the Fan, Light & door
5. I have implemented the connections’ like as following
6. Finally, I have checked the result by browsing from a laptop’s web browser & put the right ip into it.

Screenshots

